**New IPB™ Weatherproofing Kits from Times Microwave Systems**

Times Microwave Systems has introduced its new **IPB™** weatherproofing system for both long term outdoor deployments and mission critical short term deployments. The **IPB™** boots come in two different interface sizes (N and 7/16 DIN). The “N” boots will cover anything smaller than a mini DIN. Boots are sized for a particular cable and are available with either male or female threads. Boots are available for LMR-400 and 600 as well as ¼” and ½” helically corrugated cables, and ½” and 7/8” annularly corrugated cables. O-rings are available for N and 7/16 DIN female bulkheads which can be used with any of the male cable boots.

for LMR-400 connectors. The **IPB™** boots are IP68 rated and both RoHS and REACH compliant.

Part Number Stock Code Description List Price

IPB-400-NM 3109-417-1 LMR-400 Male IP boot for type N, TNC, BNC, 4310,4195 $12.00

IPB-400-NF 3109-417-2 LMR-400 Female IP boot for type N, TNC, BNC, 4310,4195 $12.00

IPB-400-NM-RA 3109-417-3 LMR-400 Male IP boot right angle for type N, TNC, BNC, 4310,419 $16.00

IPB-600-NM 3109-417-4 LMR-600 Male IP boot for type N, TNC, BNC, 4310,4195 $12.00

IPB-600-NF 3109-417-5 LMR-600 Female IP boot suitable for type N, TNC, BNC, 4310,4195 $12.00

IPB-600-NM-RA 3109-417-6 LMR-600 Male IP boot right angle for type N, TNC, BNC, 4310,4195 $16.00

IPB-OR NF 3109-417-7 Antenna port O-ring IP boot for type N female $4.00

IPB-250-NM 3109-417-8 FSJ1 (SPO-250) Male IP boot for type N, TNC, BNC, 4310,4195 $12.00

IPB-250-NM-RA 3109-417-9 FSJ1 (SPO-250) Male IP boot right angle for type N, TNC, BNC, 4310,4195 $16.00

IPB-250-DM 3109-417-10 FSJ1 (SPO-250) Male IP boot for type DIN 7/16 connector $12.00

IPB-250-DM-RA 3109-417-11 FSJ1 (SPO-250) Male IP boot right angle for type DIN 7/16 connector $16.00

IPB-500-NM 3109-417-12 LDF4 (LPO-500) Male IP boot for type N, TNC, BNC, 4310,4195 $12.00

IPB-500-NM-RA 3109-417-13 LDF4 (LPO-500) Male IP boot right angle for type N, TNC, BNC, 4310,4195 $16.00

IPB-500-DM 3109-417-14 LDF4 (LPO-500) Male IP boot for type DIN 7/16 connector $12.00

IPB-500-DM-RA 3109-417-15 LDF4 (LPO-500) Male IP boot right angle for type DIN 7/16 connector $16.00

IPB-LPO-500-NM 3109-417-16 LDF4 (LPO-500) Male IP boot for type N, TNC, BNC, 4310,419 $12.00

IPB-LPO-500-NM-RA 3109-417-17 LDF4 (LPO-500) Male IP boot right angle for type N, TNC, BNC, 4310,4195 $16.00

IPB-LPO-500-DM 3109-417-18 LDF4 (LPO-500) Male IP boot for type DIN 7/16 connector $12.00

IPB-LPO-500-DM-RA 3109-417-19 LDF4 (LPO-500) Male IP boot right angle for type DIN 7/16 connector $16.00

IPB-LPO-875-DF 3109-417-20 LDF5 (LPO-875) Female IP boot for type DIN 7/16 connector $12.00

IPB-OR-DF 3109-417-21 Antenna port O ring IP boot for DIN 7/16 female $4.00

**About Times Microwave Systems**

Times Microwave Systems has over 65 years experience in designing innovative, high-reliability, coaxial cables and assemblies for demanding interconnection problems. An engineering oriented organization, the company specializes in the design and manufacture of high performance flexible and semi-rigid coaxial cable, connectors, and cable assemblies for RF transmission from HF through microwave frequencies as well as surge arrestors for the protection of RF equipment.

**For further information contact:**

**Carolyn Turner**: Marketing Coordinator, Times Microwave Systems

Tel.: +1 203 949 8429, Email: [carolyn.turner@timesmicro.com](mailto:carolyn.turner@timesmicro.com)

**Kevin Moyher**: Product Manager, Times Microwave SystemsTel.: +1 203 949 8447, Email: [Kevin.moyher@timesmicro.com](mailto:Kevin.moyher@timesmicro.com)